BLowPass4 24db/oct rolloff - 4th order resonant Low Pass Filter. [1]

BLowPass4.ar(in, freq, rq, mul, add)

in - input signal to be processed

freq - cutoff frequency.

rq - the reciprocal of Q. bandwidth / cutoffFreq.

The B equalization suite is based on the Second Order Section (SOS) biquad UGen.

note: Biquad coefficient calculations imply certain amount of CPU overhead. These plugin UGens contain optimizations such that the coefficients get updated only when there has been a change to one of

the filter's parameters. This can cause spikes in CPU performance and should be considered when using several of these units.

[1] this is a composite pseudo UGen. BLowPass4 is built by cascading 2 SOS sections.

see also: SOS, BLowPass, BHiPass, BHiPass4, BPeakEQ, BLowShelf, BHiShelf, BBandPass, BBandStop, BAllPass.

s.boot;

(

z = {

BLowPass4.ar(

SoundIn.ar([0,1]),

MouseX.kr(10,20000,\exponential), // cutoff freq.

MouseY.kr(0.1, 1.0, \linear), // rq - compensate for 2 biquad sections.

0.5); // mul

}.play)

z.release;