GbmanL gingerbreadman map chaotic generator

GbmanL.ar(freq, xi, yi, mul, add)

GbmanL.kr(freq, xi, yi, mul, add)

freq - iteration frequency in Hertz

xi - initial value of x

yi - initial value of y

A linear-interpolating sound generator based on the difference equations:

xn+1 = 1 - yn + |xn|

yn+1 = xn

The behavior of the system is dependent only on its initial conditions and cannot

be changed once it's started.

Reference:

Devaney, R. L. "The Gingerbreadman." Algorithm 3, 15-16, Jan. 1992.

// default initial params

{ GbmanL.ar(MouseX.kr(20, SampleRate.ir)) * 0.1 }.play(s);

// different initial params

{ GbmanL.ar(MouseX.kr(20, SampleRate.ir), -0.7, -2.7) * 0.1 }.play(s);

// wait for it...

{ GbmanL.ar(MouseX.kr(20, SampleRate.ir), 1.2, 2.0002) * 0.1 }.play(s);

// as a frequency control

{ SinOsc.ar(GbmanL.ar(40)*400+500)*0.4 }.play(s);